Need to test/diagnose:

Figure out why USB circuit is non-operational

Audio Line In

* Mic In

Ethernet

SD Card

All led outputs

Need to change:

Power socket on power distro board is mirrored.

Should put LED GPIO by screw terminals.

Can’t see led connection labels (+, -, d) with terminals installed.

5v connection needs to be made to pins 23 and 24 of U$14

Come up with a better solution for programing port

* Larger pads
* Small pin headers

Want onboard LEDs

* 3v3 Power LED with jumper pads
* USB data LEDs

Need to work on:

Organize file sys.

* Put the board files on Git

Create a board info file to distribute for quotes